Name: Id#

COE 202, Term 132

Digital Logic Design
Quiz# 5

 Date: Tuesday, May 6

#

Question 1. (**13 points)**

1. In the circuit shown, A is a D-type latch and B is a D-type flip flop. For the input waveforms given for the clock signal (Clk) and the input X, accurately draw the resulting waveforms at outputs **QA** and **QB**.

Assume that both QA and QB are initially at 0.





1. The state diagram shown is for a sequential circuit that has a single input X and a single output Y. The circuit uses two positive edge triggered D-type flip flops Q1 and Q0.
2. Starting with the circuit in state Q1Q0=11, complete the missing waveforms in the timing diagram below.



1. Let the circuit be in state 00 with input X held permanently at 0. The circuit will end up being stuck at state \_\_\_\_\_\_\_. With the circuit operating at a clock frequency of 2 KHz, this state transition takes a minimum time duration of \_\_\_\_\_\_\_ ms.

**Question 2. (12 Points)**

Consider the sequential circuit opposite and then answer the following questions:

a. Is the circuit Mealy or Moore?

b. Provide logical expressions for the flip flop D inputs and the external output

c. Give both the **state table** and the **state diagram**. Use the layout given below for the state diagram. Note: Q0 represents the LSB of the binary value of the state.

