Name: KEY Id#

COE 202, Term 112

Digital Logic Design

Quiz# 6

 Date: Monday, May 7

#

# **Q1**. It is required to design a sequential circuit that receives a serial input X, and produces a serial output Z, equivalent to 3\*X, i.e., Z=3\*X. The state diagram for this circuit is shown below:

S1

S2

S0

1/1

0/0

0/1

0/0

1/0

1/1

## Show the state table of the sequential circuit.

|  |  |  |  |
| --- | --- | --- | --- |
| Current State | Input (X) | Next State | Output (Z) |
| S0 | 0 | S0 | 0 |
| S0 | 1 | S1 | 1 |
| S1 | 0 | S0 | 1 |
| S1 | 1 | S2 | 0 |
| S2 | 0 | S1 | 0 |
| S2 | 1 | S2 | 1 |

## Implement the sequential circuit using D-FFs and the smallest number of gates possible assuming the state assignment: S0=00, S1=01, and S2=10. Minimize your equations using K-map method.

## Draw the circuit diagram.

We need two flip flops to implement the design F1 and F0.

Transition Table:

|  |  |  |  |
| --- | --- | --- | --- |
| Current State (F1 F0) | Input (X) | Next State (F1 F0) | Output (Z) |
| 00 | 0 | 00 | 0 |
| 00 | 1 | 01 | 1 |
| 01 | 0 | 00 | 1 |
| 01 | 1 | 10 | 0 |
| 10 | 0 | 01 | 0 |
| 10 | 1 | 10 | 1 |
| 11 | 0 | xx | x |
| 11 | 1 | xx | x |

|  |  |
| --- | --- |
|  D1 = F1 X + F0 X = X (F1 + F0) |   D0 = F1 X’ + F1’ F0’ X |
|   Z = F0’ X + F0 X’ = F0 ⊕ X |  |

# **Q2**. It is required to design a sequential circuit that receives a serial input X and produces a serial output Z. The output Z will be 1 when the circuit detects the sequence 10010 assuming overlapping sequence detection.

# Derive the state diagram for your circuit assuming Mealy model.



# Derive the state diagram for your circuit assuming Moore model.

