Name: KEY Id#

COE 205, Term 101

Computer Organization & Assembly Programming

Quiz#2

 Date: Wednesday, Oct. 20, 2010

#

# **Q1.** Fill the blank in each of the following:

#  The address bus of the Pentium IV processor is 36 bits while the data bus is 64 bits.

# Characteristics of RISC processors include small and simple instruction set and all instructions have the same width.

# Characteristics of CISC processors include large and complex instruction set and variable width instructions.

# The Pentium IV processor has 8 32-bit general purpose registers, namely EAX, EBX, ECX, EDX, ESP, EBP, ESI, EDI.

# The Instruction Pointer (EIP) register holds the address of the next instruction to be fetched from memory.

# Each machine language instruction is first fetched from the memory and stored in an instruction register (IR).

#

# Assuming that EIP=0000101F, after fetching a 5-byte instruction EIP= 0000101F+5=00001024.

# Assuming one clock cycle per pipeline stage, executing 100 instructions in an 8-stage pipeline without any pipeline interruptions will take 8+99=107 cycles.

# Assuming real mode and that IP=20E5, CS=03FC, the linear address of the next instruction to be fetched from memory is 03FC0+20E5=060A5.

# Suppose that all segments from seg#0 until seg#100 are used. The segment number that will be allocated for a 3 Kbyte code segment is 101 and for a 1 Kbyte data segment is 1C1.

#  Segment unit translates logical address to linear address using segment descriptor table.

#  Paging unit translates linear address to physical address using a page directory and a page table