***King Fahd University of Petroleum and Minerals***

***College of Computer Science and Engineering***

***Computer Engineering Department***

COE 301 COMPUTER ORGANIZATION

**ICS 233: COMPUTER ARCHITECTURE & ASSEMBLY LANGUAGE**

**Term 151 (Fall 2015-2016)**

**Major Exam 1**

**Saturday Oct. 10, 2015**

**Time: 120 minutes, Total Pages: 9**

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ID:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Section: \_\_\_\_\_\_\_**

**Notes:**

* Do not open the exam book until instructed
* Answer all questions
* All steps must be shown
* Any assumptions made must be clearly stated

|  |  |  |
| --- | --- | --- |
| **Question** | **Max Points** | **Score** |
| **Q1** | **35** |  |
| **Q2** | **25** |  |
| **Total** | **60** |  |

Dr. Aiman El-Maleh

Dr. Mayez Al-Muhammad

# **[35 Points]**

# **(Q1)** Fill in the blank in each of the following questions:

## Assuming 12-bit unsigned representation, the binary number 1111 0000 1111 is equal to the decimal number \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## Assuming 12-bit signed 2`s complement representation, the hexadecimal number FC0 is equal to the decimal number \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## Accessibility to hardware resources is an advantage of programming in \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ language.

## Code portability is an advantage of programming in \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ language.

## With a 36-bit address bus and 64-bit data bus, the maximum memory size (assuming byte addressable memory) that can be accessed by a processor is \_\_\_\_\_\_\_\_\_\_\_ and the maximum number of bytes that can be read or written in a single cycle is \_\_\_\_\_\_\_\_\_\_\_\_.

## The bandwidth mismatch between the speed of processor and the speed of main-memory is alleviated by using \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## The advantage of dynamic RAM over static RAM is that it is \_\_\_\_\_\_\_\_\_\_ and \_\_\_\_\_\_\_\_\_\_ but the disadvantage is \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## The instruction set architecture of a processor consists of \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## Assuming that the CPU has just read a 32-bit MIPS instruction from the address 0x00400008. Then, the address of the next instruction that this CPU is going to read is\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## Given a magnetic disk with the following properties:

* Time of one rotation is 8 ms
* Average seek = 8 ms, Sector = 512 bytes, Track = 200 sectors

The average time to access a block of 20 consecutive sectors is \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ms.

## The pseudo instruction *neg $s2, $s1 (*$s2 is computed as the negative value of $s1)is implemented by the following minimum MIPS instructions:

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## The pseudo instruction *ble $s2, $s1, Next* is implemented by the following minimum MIPS instructions:

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## The pseudo instruction *rol $s0, $s0, 8 (*$s0 is rotated to the left by 8 bits and stored in $s0) is implemented by the following minimum MIPS instructions:

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## Assuming that $a0 contains an Alphabetic character, the instruction *\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_* will guarantee that the character in $a0 is an upper case character. Note that the ASCII code of character ‘A’ is 0x41 while that of character ‘a’ is 0x61.

## Assume that the instruction *bne $t0, $t1, NEXT* is at address 0x00400020 in the text segment, and the label NEXT is at address 0x00400010. Then, the address stored in the assembled instruction for the label NEXT is \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

## Assuming that variable Array is defined as shown below:

Array: .byte 1, 2, -3, 4

After executing the following sequence of instructions, the content of the three registers is $t1=\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, $t2=\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_, and $t3=\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_.

la $t0, Array

lb $t1, 2($t0)

lh $t2, 2($t0)

lw $t3, 0($t0)

## Assuming the following data segment, and assuming that the first variable X is given the address **0x10010000**, then the addresses for variables Y and Z will be \_\_\_\_\_\_\_\_\_\_\_\_\_ and \_\_\_\_\_\_\_\_\_\_\_\_\_.

## .data

## X: .byte 1

## Y: .half 2, 3

## Z: .word 4

## To multiply the **signed** content of register $t0 by 127.75 without using multiplications and division instructions, we use the following MIPS instructions:

## \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## The condition for which the data stored in $t0 must satisfy in order for the following MIPS fragment to branch to L1 is:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ori $t1, $0, 0x111

and $t0, $t0, $t1

beq $t0, $t1, L1

## The content of register **$t0** after executing the following code is \_\_\_\_\_\_\_\_\_\_:

li $s1, 0x4321

xor $t0, $t0, $t0

Next:

andi $t1, $s1, 0xf

add $t0, $t0, $t1

srl $s1, $s1, 4

bne $s1, $0, Next

**[25 Points]**

# **(Q2)** Write separate MIPS assembly code fragments with **minimum** instructions to implement each of the given requirements.

## [6 points] Given two arrays of words A and B with their base addresses stored in registers $s0 and $s1, array size N is stored in $s2, and index i is stored $s3, write the smallest MIPS assembly fragment for the following computation:

# **for (i=0; i<n; i++) if ( (A[i]-B[i])\*5 >=0 ) then A[i]= (A[i]-B[i])\*5;**

## [6 points] Given the following MIPS assembly fragment:

**bne $s1, $s2, exit**

**bge $s2, $s3, exit**

**addi $s4, $s4, 5**

**Exit:**

Assume that variables a, b, c, and d are stored in registers $s1, $s2, $s3, and $s4, respectively.

Fill in the Boolean expression in the following IF statement:

If ( \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_) then d=d +5;

Repeat the above question for the following MIPS assembly fragment:

**beq $s1, $s2, process**

**bgt $s2, $s3, exit**

**ble $s3, $s4, exit**

**process: add $s4, $s4, $s1**

**Exit:**

Fill in the Boolean expression in the following IF statement:

If (­­­­­­­­­­­­­­­­­­­­­­­­­­­­­­­\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_) then d=d +a;

## [3 points] Write a MIPS assembly fragment for the following IF statement:

## **if ( [(a == b) || ( c== d) ] && (a < c) ) then b = d ;**

## Assume that variables a, b, c, and d are stored into registers $s0, $s1, $s2, and $s3, respectively.

## [5 points] Write a MIPS assembly fragment to count the number of occurrence of alphabetic characters (can be lowercase or uppercase) in a null terminated string, where the base address of the string is in register $s0 and the count is to be in $s1**.**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | A | B | C | D | E | F |
| 2 | space | **!** | **"** | **#** | **$** | **%** | **&** | **'** | **(** | **)** | **\*** | **+** | **,** | **-** | **.** | **/** |
| 3 | **0** | **1** | **2** | **3** | **4** | **5** | **6** | **7** | **8** | **9** | **:** | **;** | **<** | **=** | **>** | **?** |
| 4 | **@** | **A** | **B** | **C** | **D** | **E** | **F** | **G** | **H** | **I** | **J** | **K** | **L** | **M** | **N** | **O** |
| 5 | **P** | **Q** | **R** | **S** | **T** | **U** | **V** | **W** | **X** | **Y** | **Z** | **[** | **\** | **]** | **^** | **\_** |
| 6 | **`** | **a** | **b** | **c** | **d** | **e** | **f** | **G** | **h** | **i** | **j** | **k** | **l** | **m** | **n** | **o** |
| 7 | **p** | **q** | **r** | **s** | **t** | **u** | **v** | **W** | **x** | **y** | **z** | **{** | **|** | **}** | **~** | DEL |

## [5 points] Write the most optimized MIPS assembly fragment for the following WHILE statement:

## 

## **i = 0;**

## **WHILE ( (A[i] >= B[i]\*2) && (i<N) ) { A[i] = A[i]- B[i]; i = i+1; }**

Where A and B are arrays of Bytes. The base addresses of arrays A and B are stored into registers $s0 and $s1, respectively. The index i and count N are stored into registers $s2 and $s3.

**MIPS Instructions:**













