***King Fahd University of Petroleum and Minerals***

***College of Computer Science and Engineering***

***Computer Engineering Department***

COE 301 COMPUTER ORGANIZATION

**ICS 233: COMPUTER ARCHITECTURE & ASSEMBLY LANGUAGE**

**Term 151 (Fall 2015-2016)**

**Major Exam 2**

**Saturday Nov. 21, 2015**

**Time: 120 minutes, Total Pages: 15**

**Name:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ID:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Section: \_\_\_\_\_\_\_**

**Notes:**

* Do not open the exam book until instructed
* Answer all questions
* All steps must be shown
* Any assumptions made must be clearly stated

|  |  |  |
| --- | --- | --- |
| **Question** | **Max Points** | **Score** |
| **Q1** | **16** |  |
| **Q2** | **20** |  |
| **Q3** | **20** |  |
| **Q4** | **30** |  |
| **Total** | **86** |  |

Dr. Aiman El-Maleh

Dr. Mayez Al-Muhammad

# **[16 Points]**

# **(Q1)**

## **[6 points]** A recursive procedure TH(N) returns 1+2TH(N-1) for N >1, 1 if N=1, and zero otherwise. This is called Tower of Hanoi. TH(N) is defined as follows:

int TH(int N) {

if (N =< 0) return 0;

else if (N=1) return 1;

else return (1 + 2\*TH(N-1));

}

Assume TH receives its argument N in register $a0 and return its results in $v0. The above procedure is called from some Main program, which needs not to be implemented here. Write a minimal MIPS program for the above procedure.

## **[10 points]** Suppose we enter i integers q(1), q(2), …, q(i). The objective is to compute the result p(i) = q(1) +… + q(i) for each i, where p is an array of results. A better way to compute the results is p(i) = p(i-1)+ q(i) for i >=1 after setting p(0)=0. The above function is called prefix sum. For example, if we enter 4, 3, 5, 2, 3, 0 (termination) as follows:

Order of entries 1 2 3 4 5 6

Value of entries q: 4 3 5 2 3 0 then the results will be:

Value of results p: 4 7 12 14 17

Assume the following strings in the data segments:

prompt-1: .asciiz "Please enter at most 100 singed integers terminating with 0: \n"

prompt-2: .asciiz "Prefix sum of the entered integers: \n"

Use $s0 to store the address of array of words p as a base address and $s1 to store the number of entered integers by the user.

Write a MIPS program with minimal instructions that carries out the following steps:

1. Print “prompt-1”,

2. Reads at most 100 signed integers q(i) terminated with a zero,

3. Compute the results p(i) and store them in memory,

4. Print “prompt-2”, and

5. Print all the results p(i).

**[20 Points]**

## **(Q2)**

## **[10 points]** You are required to design a circuit that can be used to perform **signed** multiplication of two 32-bit operands A and B. Show the block diagram of all used components and their sizes. Explain how the circuit will be used to perform signed multiplication by showing a flow chart or pseudo code.

## **[4 points]** Given that **Multiplicand=1001** and **Multiplier=1011,** using the **signed multiplication** hardware, show the **signed** multiplication of **Multiplicand** by **Multiplier**. The result of the multiplication should be an 8 bit **signed** number in HI and LO registers. Show the steps of your work.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Iteration** | | **Multiplicand** | **Sign** | **Product = HI,LO** |
| 0 | Initialize |  |  |  |
| 1 |  |  |  |  |
|  |  |  |  |
| 2 |  |  |  |  |
|  |  |  |  |
| 3 |  |  |  |  |
|  |  |  |  |
| 4 |  |  |  |  |
|  |  |  |  |

## **[6 points]** Given that **Dividend=1001** and **Divisor=0011** represent two **4-bit signed numbers in 2's complement representation**, using the **unsigned division** hardware, show the **signed** division of **Dividend** by **Divisor**. The result of division should be stored in the Remainder and Quotient registers. Show the steps of your work.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Iteration** | | **Remainder (HI)** | **Quotient (LO)** | **Divisor** | **Difference** |
| 0 | Initialize |  |  |  |  |
| 1 |  |  |  |  |  |
|  |  |  |  |  |
| 2 |  |  |  |  |  |
|  |  |  |  |  |
| 3 |  |  |  |  |  |
|  |  |  |  |  |
| 4 |  |  |  |  |  |
|  |  |  |  |  |

**[20 Points]**

# **(Q3)**

1. **[2 Points]** What is the **decimal value** of following single precision float:

[1, 1000 0101, 0101 1101 0000 0000 0000 000]

1. **[2 Points]** What is the **decimal value** of following single precision float:

[0, 0000 0000, 0100 0000 0000 0000 0000 000]

1. **[3 Points]** Find the normalized single precision float representation of +59.25.
2. **[4 Points]** Round the given single precision float with the given GRS bits using the following rounding modes showing the resulting normalized number:

**GRS**

**-1.111 1111 1111 1111 1111 1111 100 x 223**

Zero: [ ]

+infinity: [ ]

-infinity: [ ]

Nearest Even: [ ]

1. **[5 Points]** Find the normalized difference between A and B by using rounding to nearest even. Perform the operation using **guard**, **round** and **sticky** bits:

A= + 1.00000000000000000000000 × 24

B = +1.11110000000000000000001 × 23

1. **[4 Points]** Find the normalized result of the operation A+B+C, by performing A+B first followed by adding C, using rounding to nearest even. Perform the operation using **guard**, **round** and **sticky** bits:

A= + **1.011 1110 0100 0000 0000 0000 000 x 232**

B = +**1.111 1000 0000 0000 0000 0000 000 x 24**

C = - **1.011 1110 0100 0000 0000 0000 000 x 232**

Is the obtained result intuitive? Justify your answer.

**[30 Points]**

# **(Q4)**

## **[3 Points]** The components of a Single Cycle Datapath have the following delays**:**

1. 150 ps for fetching the instruction from the Instruction Memory,
2. 100 ps for reading or writing the register file (in parallel with instruction decoding),
3. 50 ps for any ALU operation,
4. 200 ps for loading or storing using the data memory.

The datapath setup time is 30 ps, the hold time is 45 ps, and the clock skew time is 20 ps. Ignore the delay through the multiplexers and other logic. What is the shortest clock period for correct operation of MIPS assembly instructions. Evaluate the highest possible clock rate.

## Consider the following MIPS datapath:



1. **[8 Points]** List the values of the datapath control signals in the following Table for each instruction.

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Type** | **Instr.** | **OPCODE**  X5 X4X3 X2 X1 X0 | **RegDst** | **RegWrite** | **Ext** | **ALUSrc** | **ALUCtrl** | **MemRead** | **MemWrite** | **MemtoReg** |
| **R** | **Sub** | **000001** |  |  |  |  |  |  |  |  |
| **Or** | **000010** |  |  |  |  |  |  |  |  |
| **I** | **Addi** | **000100** |  |  |  |  |  |  |  |  |
| **Andi** | **000111** |  |  |  |  |  |  |  |  |
| **Lw** | **001000** |  |  |  |  |  |  |  |  |
| **Sw** | **001001** |  |  |  |  |  |  |  |  |
| **Beq** | **001100** |  |  |  |  |  |  |  |  |
| **J** | **J** | **001110** |  |  |  |  |  |  |  |  |

1. **[4 Points]** Design the control unit to generate the above control signals (except ALUCtrl) using the simplest logic.

## **[5 Points]** We would like to add a new instruction to the MIPS instruction set: **Addm rd, rt, rs** that performs (rd) 🡨 DM[(rs)]+(rt). Draw the additional changes on the MIPS datapath shown below to enable the execution of Addm instruction and give the values of all the control signals in the modified datapath by filling the given table.



|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **RegDst** | **RegWrite** | **Ext** | **ALUSrc** | **ALUCtrl** | **MemRead** | **MemWrite** | **MemtoReg** |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

## **[5 Points]** Assume we want to add instructions to MIPS such as: Addp rd, rt, rs that performs (rd) 🡨 (rs)+(rt) if $R23=1, else register rd remains unchanged. This is called a predicated instruction that executes only if a predicate is true (register $R23=1). We assume that:

1. Control signals generated by the control unit for Addp are identical to those generated for Add rd, rt, rs instruction.
2. The Control unit generates a signal S=1 only for predicated instructions.
3. The content of register $R23 is always output by the Registers (see the below drawing).

Draw the additional changes on the MIPS datapath to enable correct execution of Addp instruction and give the values of all the control signals in the modified datapath by filling the given table.




|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **RegDst** | **RegWrite** | **Ext** | **ALUSrc** | **ALUCtrl** | **MemRead** | **MemWrite** | **MemtoReg** |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |

## **[5 Points]** Assume that we want to add the instruction JAL to the MIPS datapath. Make all the necessary modifications to the MIPS Datapath for implementing the JAL instruction including the NextPC block. The NextPC block implementation is given below.





**Syscall Services:**



**MIPS Instructions:**

