Name: KEY Id#

COE 405, Term 152


Design & Modeling of Digital Systems

Quiz# 3

Date: Sunday, April 3, 2016


# **Q1**. Given below the design of an *n*-bit magnitude comparator. The circuit receives two *n*-bit unsigned numbers ***A*** *and* ***B*** and produces two outputs **GT** and **EQ** as given in the table to the right.

|  |  |
| --- | --- |
|  | **GT EQ** |
| IF A > B | 1 0 |
| IF A = B | 0 1 |
| IF A < B | 0 0 |




# The input operands are processed in a bitwise manner *starting with the most significant bit (MSB)*. The comparator circuit is constructed using *n identical copies* of the basic 1-bit *cell* shown to the right.

# The Figure below shows the *n*-bit comparator circuit implemented using *n* copies of the basic 1-bit cell.



# Boolean expressions of the outputs of ***cell i*** and its gate-level implementation are given below:



Cell *i* Gate Level Implementation

*EQi =* (*Ai* 🞊 *Bi*). *EQi+1*

## Write a Verilog model **Comp1Bit** to model the 1-bit comparator circuit using *either* a structural model of basic logic gates *or* a behavioral model using the **assign** statement.

The declaration of the Comp1Bit module is as follows:

**module** Comp1Bit **(output** GT\_out, EQ\_out , **input** GT\_in , EQ\_in, Ai, Bi**);**

module Comp1Bit (output GT\_out, EQ\_out, input GT\_in, EQ\_in, Ai, Bi);

assign GT\_out = GT\_in || Ai && !Bi && EQ\_in;

assign EQ\_out = (Ai ~^ Bi) && EQ\_in;

endmodule

OR

module Comp1Bit (output GT\_out, EQ\_out, input GT\_in, EQ\_in, Ai, Bi);

not (g1, Bi);

and (g2, g1, Ai);

xnor(g3, Ai, Bi);

and (g4, g2, EQ\_in);

or (GT\_out, GT\_in, g4);

and (EQ\_out, EQ\_in, g3);

endmodule

## Complete the following Verilog model **Comp3Bit** that models a 3-bit comparator circuit.

module Comp3Bit (output Greater, Equal,

input [2:0] A , B) ;

wire [2:1] GT, EQ ; // internal wires connecting cells

/\* First instance “M1” of the cell Comp1Bit with its inputs GT\_in and EQ\_in connected to fixed values of 0 and 1 respectively \*/

//

Comp1Bit M1 (GT[2] , EQ [2], 1'b0, 1'b1, A[2], B[2]);

Comp1Bit M2 (GT[1], EQ[1], GT[2], EQ[2], A[1], B[1]);

Comp1Bit M3 (Greater, Equal, GT[1], EQ[1], A[0], B[0]);

endmodule

## Write a Verilog test bench to test the 3-bit comparator **Comp3Bit** by applying the following input patterns consecutively with a delay of 20ps:

## {A=100, B=011},

## {A=101, B=101},

## {A=011, B=111}.

module t\_Comp3Bit();

wire Greater, Equal;

reg [2:0] A, B;

Comp3Bit M1 (Greater, Equal, A, B) ;

initial begin

A=3'b100; B=3'b011;

#20 A=3'b101; B=3'b101;

#20 A=3'b011; B=3'b111;

end

endmodule