Name: Id#

COE 301/ICS 233, Term 172

Computer Architecture & Assembly Language

Quiz# 6

 Date: Tuesday, April 17, 2018

# **Q1.** Consider the single-cycle datapath and control given below along with ALU design for the MIPS processor implementing a subset of the instruction set:





## **(5 points)** Show the control signals generated for the execution of the following instructions by filling the table given below:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Op | RegDst | RegWrite | ExtOp | ALUSrc | MemRead | MemWrite | WBdata |
| R-type |  |  |  |  |  |  |  |
| xori |  |  |  |  |  |  |  |
| lw |  |  |  |  |  |  |  |
| bne |  |  |  |  |  |  |  |
| j  |  |  |  |  |  |  |  |

## **(4 points)** Show the block diagram for designing the main control unit for this CPU and show the logic gates or equations for the control signals **RegDst**, **RegWrite** and **ExtOp** based on these instructions. Assume that the opcode of these instructions is a 6-bit opcode such that the opcode for R-type instructions is 0, the opcode for xori is 1, the opcode for lw is 2, and so on for the rest of the instructions.

## **(12 points)** We wish to add the following instructions to the MIPS single-cycle datapath. Add any necessary datapath modifications and control signals needed for the implementation of these instructions. Show only the **modified** and **added** components to the datapath.

* 1. srl
	2. lui
	3. bgtz
	4. jal